<?xml version="1.0" encoding= "UTF-8" ?>
<configuration name="MIMXRT1176xxxxx" xsi:schemaLocation="http://mcuxpresso.nxp.com/XSD/mex_configuration_17 http://mcuxpresso.nxp.com/XSD/mex_configuration_17.xsd" uuid="060646c1-2247-47a8-b52d-03c1968b4426" version="17" xmlns="http://mcuxpresso.nxp.com/XSD/mex_configuration_17" xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance">
   <common>
      <processor>MIMXRT1176xxxxx</processor>
      <package>MIMXRT1176DVMAA</package>
      <board>MIMXRT1170-EVKB</board>
      <mcu_data>ksdk2_0</mcu_data>
      <cores selected="cm7">
         <core name="Cortex-M4F" id="cm4" description=""/>
         <core name="Cortex-M7F" id="cm7" description=""/>
      </cores>
      <description>Configuration imported from evkbmimxrt1170_dev_cdc_vcom_lite_bm_cm7</description>
   </common>
   <preferences>
      <validate_boot_init_only>true</validate_boot_init_only>
      <generate_code_modified_registers_only>false</generate_code_modified_registers_only>
      <update_include_paths>true</update_include_paths>
      <generate_registers_defines>false</generate_registers_defines>
   </preferences>
   <tools>
      <pins name="Pins" version="17.0" enabled="true" update_project_code="true">
         <generated_project_files>
            <file path="board/pin_mux.c" update_enabled="true"/>
            <file path="board/pin_mux.h" update_enabled="true"/>
         </generated_project_files>
         <pins_profile>
            <processor_version>24.12.10</processor_version>
            <pin_labels>
               <pin_label pin_num="M13" pin_signal="GPIO_AD_04" label="SIM1_PD/J44[C8]/USER_LED_CTL1/J9[8]/J25[7]" identifier="SIM1_PD;LED;USER_LED"/>
            </pin_labels>
            <external_user_signals>
               <properties/>
            </external_user_signals>
            <power_domains/>
         </pins_profile>
         <functions_list>
            <function name="BOARD_InitPins">
               <description>Configures pin routing and optionally pin electrical features.</description>
               <options>
                  <callFromInitBoot>true</callFromInitBoot>
                  <coreID>cm7</coreID>
                  <enableClock>true</enableClock>
               </options>
               <dependencies>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Pins initialization requires the COMMON Driver in the project." problem_level="2" source="Pins:BOARD_InitPins">
                     <feature name="enabled" evaluation="equal" configuration="cm7">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.iomuxc" description="Pins initialization requires the IOMUXC Driver in the project." problem_level="2" source="Pins:BOARD_InitPins">
                     <feature name="enabled" evaluation="equal" configuration="cm7">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.igpio" description="Pins initialization requires the IGPIO Driver in the project." problem_level="2" source="Pins:BOARD_InitPins">
                     <feature name="enabled" evaluation="equal" configuration="cm7">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <pins>
                  <pin peripheral="GPIO9" signal="gpio_io, 03" pin_num="M13" pin_signal="GPIO_AD_04">
                     <pin_features>
                        <pin_feature name="identifier" value="USER_LED"/>
                        <pin_feature name="direction" value="OUTPUT"/>
                        <pin_feature name="pull_up_down_config" value="Pull_Down"/>
                        <pin_feature name="pull_keeper_select" value="Keeper"/>
                     </pin_features>
                  </pin>
                  <pin peripheral="GPIO13" signal="gpio_io, 00" pin_num="T8" pin_signal="WAKEUP">
                     <pin_features>
                        <pin_feature name="direction" value="INPUT"/>
                        <pin_feature name="pull_up_down_config" value="Pull_Up"/>
                     </pin_features>
                  </pin>
               </pins>
            </function>
            <function name="BOARD_InitDEBUG_UARTPins">
               <description>Configures pin routing and optionally pin electrical features.</description>
               <options>
                  <callFromInitBoot>true</callFromInitBoot>
                  <coreID>cm7</coreID>
                  <enableClock>true</enableClock>
               </options>
               <dependencies>
                  <dependency resourceType="Peripheral" resourceId="LPUART1" description="Peripheral LPUART1 signals are routed in the Pins Tool, but the peripheral is not initialized in the Peripherals Tool." problem_level="1" source="Pins:BOARD_InitDEBUG_UARTPins">
                     <feature name="initialized" evaluation="equal">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Pins initialization requires the COMMON Driver in the project." problem_level="2" source="Pins:BOARD_InitDEBUG_UARTPins">
                     <feature name="enabled" evaluation="equal" configuration="cm7">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.iomuxc" description="Pins initialization requires the IOMUXC Driver in the project." problem_level="2" source="Pins:BOARD_InitDEBUG_UARTPins">
                     <feature name="enabled" evaluation="equal" configuration="cm7">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <pins>
                  <pin peripheral="LPUART1" signal="TXD" pin_num="L13" pin_signal="GPIO_AD_24">
                     <pin_features>
                        <pin_feature name="pull_keeper_select" value="Keeper"/>
                        <pin_feature name="slew_rate" value="Slow"/>
                     </pin_features>
                  </pin>
                  <pin peripheral="LPUART1" signal="RXD" pin_num="M15" pin_signal="GPIO_AD_25">
                     <pin_features>
                        <pin_feature name="pull_keeper_select" value="Keeper"/>
                        <pin_feature name="slew_rate" value="Slow"/>
                     </pin_features>
                  </pin>
               </pins>
            </function>
         </functions_list>
      </pins>
      <clocks name="Clocks" version="15.0" enabled="true" update_project_code="true">
         <generated_project_files>
            <file path="board/clock_config.c" update_enabled="true"/>
            <file path="board/clock_config.h" update_enabled="true"/>
         </generated_project_files>
         <clocks_profile>
            <processor_version>24.12.10</processor_version>
         </clocks_profile>
         <clock_configurations>
            <clock_configuration name="BOARD_BootClockRUN" id_prefix="" prefix_user_defined="false">
               <description></description>
               <options/>
               <dependencies>
                  <dependency resourceType="PeripheralUnifiedSignal" resourceId="ANADIG.xtali" description="&apos;XTALI&apos; (Pins tool id: ANADIG.xtali, Clocks tool id: ANADIG_OSC.XTALI) needs to be routed" problem_level="1" source="Clocks:BOARD_BootClockRUN">
                     <feature name="routed" evaluation="">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PeripheralUnifiedSignal" resourceId="ANADIG.xtali" description="&apos;XTALI&apos; (Pins tool id: ANADIG.xtali, Clocks tool id: ANADIG_OSC.XTALI) needs to have &apos;INPUT&apos; direction" problem_level="1" source="Clocks:BOARD_BootClockRUN">
                     <feature name="direction" evaluation="">
                        <data>INPUT</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PeripheralUnifiedSignal" resourceId="ANADIG.xtalo" description="&apos;XTALO&apos; (Pins tool id: ANADIG.xtalo, Clocks tool id: ANADIG_OSC.XTALO) needs to be routed" problem_level="1" source="Clocks:BOARD_BootClockRUN">
                     <feature name="routed" evaluation="">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PeripheralUnifiedSignal" resourceId="ANADIG.xtalo" description="&apos;XTALO&apos; (Pins tool id: ANADIG.xtalo, Clocks tool id: ANADIG_OSC.XTALO) needs to have &apos;OUTPUT&apos; direction" problem_level="1" source="Clocks:BOARD_BootClockRUN">
                     <feature name="direction" evaluation="">
                        <data>OUTPUT</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PeripheralUnifiedSignal" resourceId="ANADIG.rtc_xtali" description="&apos;RTC_XTALI&apos; (Pins tool id: ANADIG.rtc_xtali, Clocks tool id: ANADIG_OSC.RTC_XTALI) needs to be routed" problem_level="1" source="Clocks:BOARD_BootClockRUN">
                     <feature name="routed" evaluation="">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PeripheralUnifiedSignal" resourceId="ANADIG.rtc_xtali" description="&apos;RTC_XTALI&apos; (Pins tool id: ANADIG.rtc_xtali, Clocks tool id: ANADIG_OSC.RTC_XTALI) needs to have &apos;INPUT&apos; direction" problem_level="1" source="Clocks:BOARD_BootClockRUN">
                     <feature name="direction" evaluation="">
                        <data>INPUT</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PeripheralUnifiedSignal" resourceId="ANADIG.rtc_xtalo" description="&apos;RTC_XTALO&apos; (Pins tool id: ANADIG.rtc_xtalo, Clocks tool id: ANADIG_OSC.RTC_XTALO) needs to be routed" problem_level="1" source="Clocks:BOARD_BootClockRUN">
                     <feature name="routed" evaluation="">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PeripheralUnifiedSignal" resourceId="ANADIG.rtc_xtalo" description="&apos;RTC_XTALO&apos; (Pins tool id: ANADIG.rtc_xtalo, Clocks tool id: ANADIG_OSC.RTC_XTALO) needs to have &apos;OUTPUT&apos; direction" problem_level="1" source="Clocks:BOARD_BootClockRUN">
                     <feature name="direction" evaluation="">
                        <data>OUTPUT</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Clocks initialization requires the COMMON Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockRUN">
                     <feature name="enabled" evaluation="equal" configuration="cm4">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.common" description="Clocks initialization requires the COMMON Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockRUN">
                     <feature name="enabled" evaluation="equal" configuration="cm7">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.iomuxc" description="Clocks initialization requires the IOMUXC Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockRUN">
                     <feature name="enabled" evaluation="equal" configuration="cm4">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.iomuxc" description="Clocks initialization requires the IOMUXC Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockRUN">
                     <feature name="enabled" evaluation="equal" configuration="cm7">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.dcdc_soc" description="Clocks initialization requires the DCDC_SOC Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockRUN">
                     <feature name="enabled" evaluation="equal" configuration="cm4">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.dcdc_soc" description="Clocks initialization requires the DCDC_SOC Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockRUN">
                     <feature name="enabled" evaluation="equal" configuration="cm7">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.pmu_1" description="Clocks initialization requires the PMU_1 Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockRUN">
                     <feature name="enabled" evaluation="equal" configuration="cm4">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.pmu_1" description="Clocks initialization requires the PMU_1 Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockRUN">
                     <feature name="enabled" evaluation="equal" configuration="cm7">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.clock" description="Clocks initialization requires the CLOCK Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockRUN">
                     <feature name="enabled" evaluation="equal" configuration="cm4">
                        <data>true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="SWComponent" resourceId="platform.drivers.clock" description="Clocks initialization requires the CLOCK Driver in the project." problem_level="2" source="Clocks:BOARD_BootClockRUN">
                     <feature name="enabled" evaluation="equal" configuration="cm7">
                        <data>true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <clock_sources/>
               <clock_outputs>
                  <clock_output id="ACMP_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="ADC1_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="ADC2_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="ARM_PLL_CLK.outFreq" value="996 MHz" locked="false" accuracy=""/>
                  <clock_output id="ASRC_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="AXI_CLK_ROOT.outFreq" value="996 MHz" locked="false" accuracy=""/>
                  <clock_output id="BUS_CLK_ROOT.outFreq" value="240 MHz" locked="false" accuracy=""/>
                  <clock_output id="BUS_LPSR_CLK_ROOT.outFreq" value="160 MHz" locked="false" accuracy=""/>
                  <clock_output id="CAN1_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="CAN2_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="CAN3_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="CCM_CLKO1_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="CCM_CLKO2_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="CLK_1M.outFreq" value="1 MHz" locked="false" accuracy=""/>
                  <clock_output id="CSI2_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="CSI2_ESC_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="CSI2_UI_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="CSI_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="CSSYS_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="CSTRACE_CLK_ROOT.outFreq" value="132 MHz" locked="false" accuracy=""/>
                  <clock_output id="ELCDIF_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="EMV1_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="EMV2_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="ENET1_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="ENET2_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="ENET_1G_TX_CLK.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="ENET_25M_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="ENET_QOS_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="ENET_TIMER1_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="ENET_TIMER2_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="ENET_TIMER3_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="FLEXIO1_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="FLEXIO2_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="FLEXSPI1_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="FLEXSPI2_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="GC355_CLK_ROOT.outFreq" value="492.0000125 MHz" locked="false" accuracy=""/>
                  <clock_output id="GPT1_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="GPT1_ipg_clk_highfreq.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="GPT2_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="GPT2_ipg_clk_highfreq.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="GPT3_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="GPT3_ipg_clk_highfreq.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="GPT4_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="GPT4_ipg_clk_highfreq.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="GPT5_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="GPT5_ipg_clk_highfreq.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="GPT6_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="GPT6_ipg_clk_highfreq.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="LCDIFV2_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="LPI2C1_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="LPI2C2_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="LPI2C3_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="LPI2C4_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="LPI2C5_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="LPI2C6_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="LPSPI1_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="LPSPI2_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="LPSPI3_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="LPSPI4_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="LPSPI5_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="LPSPI6_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="LPUART10_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="LPUART11_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="LPUART12_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="LPUART1_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="LPUART2_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="LPUART3_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="LPUART4_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="LPUART5_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="LPUART6_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="LPUART7_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="LPUART8_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="LPUART9_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="M4_CLK_ROOT.outFreq" value="4320/11 MHz" locked="false" accuracy=""/>
                  <clock_output id="M4_SYSTICK_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="M7_CLK_ROOT.outFreq" value="996 MHz" locked="false" accuracy=""/>
                  <clock_output id="M7_SYSTICK_CLK_ROOT.outFreq" value="100 kHz" locked="false" accuracy=""/>
                  <clock_output id="MIC_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="MIPI_DSI_TX_CLK_ESC_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="MIPI_ESC_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="MIPI_REF_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="MQS_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="MQS_MCLK.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="OSC_24M.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="OSC_32K.outFreq" value="32.768 kHz" locked="false" accuracy=""/>
                  <clock_output id="OSC_RC_16M.outFreq" value="16 MHz" locked="false" accuracy=""/>
                  <clock_output id="OSC_RC_400M.outFreq" value="400 MHz" locked="false" accuracy=""/>
                  <clock_output id="OSC_RC_48M.outFreq" value="48 MHz" locked="false" accuracy=""/>
                  <clock_output id="OSC_RC_48M_DIV2.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="PLL_VIDEO_CLK.outFreq" value="984.000025 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI1_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI1_MCLK1.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI1_MCLK3.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI2_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI2_MCLK1.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI2_MCLK3.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI3_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI3_MCLK1.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI3_MCLK3.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI4_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="SAI4_MCLK1.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="SEMC_CLK_ROOT.outFreq" value="198 MHz" locked="false" accuracy=""/>
                  <clock_output id="SPDIF_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="SYS_PLL2_CLK.outFreq" value="528 MHz" locked="false" accuracy=""/>
                  <clock_output id="SYS_PLL2_PFD0_CLK.outFreq" value="352 MHz" locked="false" accuracy=""/>
                  <clock_output id="SYS_PLL2_PFD1_CLK.outFreq" value="594 MHz" locked="false" accuracy=""/>
                  <clock_output id="SYS_PLL2_PFD2_CLK.outFreq" value="396 MHz" locked="false" accuracy=""/>
                  <clock_output id="SYS_PLL2_PFD3_CLK.outFreq" value="297 MHz" locked="false" accuracy=""/>
                  <clock_output id="SYS_PLL3_CLK.outFreq" value="480 MHz" locked="false" accuracy=""/>
                  <clock_output id="SYS_PLL3_DIV2_CLK.outFreq" value="240 MHz" locked="false" accuracy=""/>
                  <clock_output id="SYS_PLL3_PFD0_CLK.outFreq" value="8640/13 MHz" locked="false" accuracy=""/>
                  <clock_output id="SYS_PLL3_PFD1_CLK.outFreq" value="8640/17 MHz" locked="false" accuracy=""/>
                  <clock_output id="SYS_PLL3_PFD2_CLK.outFreq" value="270 MHz" locked="false" accuracy=""/>
                  <clock_output id="SYS_PLL3_PFD3_CLK.outFreq" value="4320/11 MHz" locked="false" accuracy=""/>
                  <clock_output id="USDHC1_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
                  <clock_output id="USDHC2_CLK_ROOT.outFreq" value="24 MHz" locked="false" accuracy=""/>
               </clock_outputs>
               <clock_settings>
                  <setting id="CoreBusClockRootsInitializationConfig" value="selectedCore" locked="false"/>
                  <setting id="SOCDomainVoltage" value="OD" locked="false"/>
                  <setting id="ANADIG_OSC_OSC_24M_CTRL_LP_EN_CFG" value="Low" locked="false"/>
                  <setting id="ANADIG_OSC_OSC_24M_CTRL_OSC_EN_CFG" value="Enabled" locked="false"/>
                  <setting id="ANADIG_PLL.PLL_AUDIO_BYPASS.sel" value="ANADIG_OSC.OSC_24M" locked="false"/>
                  <setting id="ANADIG_PLL.PLL_VIDEO.denom" value="960000" locked="false"/>
                  <setting id="ANADIG_PLL.PLL_VIDEO.div" value="41" locked="false"/>
                  <setting id="ANADIG_PLL.PLL_VIDEO.num" value="1" locked="false"/>
                  <setting id="ANADIG_PLL.SYS_PLL1_BYPASS.sel" value="ANADIG_OSC.OSC_24M" locked="false"/>
                  <setting id="ANADIG_PLL.SYS_PLL2.denom" value="268435455" locked="false"/>
                  <setting id="ANADIG_PLL.SYS_PLL2.div" value="22" locked="false"/>
                  <setting id="ANADIG_PLL.SYS_PLL2.num" value="0" locked="false"/>
                  <setting id="ANADIG_PLL.SYS_PLL2_SS_DIV.scale" value="268435455" locked="false"/>
                  <setting id="ANADIG_PLL.SYS_PLL3_PFD3_DIV.scale" value="22" locked="true"/>
                  <setting id="ANADIG_PLL.SYS_PLL3_PFD3_MUL.scale" value="18" locked="true"/>
                  <setting id="ANADIG_PLL_ARM_PLL_CTRL_POWERUP_CFG" value="Enabled" locked="false"/>
                  <setting id="ANADIG_PLL_PLL_AUDIO_CTRL_GATE_CFG" value="Disabled" locked="false"/>
                  <setting id="ANADIG_PLL_PLL_VIDEO_CTRL0_POWERUP_CFG" value="Enabled" locked="false"/>
                  <setting id="ANADIG_PLL_SYS_PLL1_CTRL0_POWERUP_CFG" value="Disabled" locked="false"/>
                  <setting id="ANADIG_PLL_SYS_PLL1_CTRL_GATE_CFG" value="Disabled" locked="false"/>
                  <setting id="ANADIG_PLL_SYS_PLL2_CTRL_POWERUP_CFG" value="Enabled" locked="false"/>
                  <setting id="ANADIG_PLL_SYS_PLL3_CTRL_POWERUP_CFG" value="Enabled" locked="false"/>
                  <setting id="ANADIG_PLL_SYS_PLL3_CTRL_SYS_PLL3_DIV2_CFG" value="Enabled" locked="false"/>
                  <setting id="CCM.CLOCK_ROOT0.MUX.sel" value="ANADIG_PLL.ARM_PLL_CLK" locked="false"/>
                  <setting id="CCM.CLOCK_ROOT1.MUX.sel" value="ANADIG_PLL.SYS_PLL3_PFD3_CLK" locked="false"/>
                  <setting id="CCM.CLOCK_ROOT2.DIV.scale" value="2" locked="false"/>
                  <setting id="CCM.CLOCK_ROOT2.MUX.sel" value="ANADIG_PLL.SYS_PLL3_CLK" locked="false"/>
                  <setting id="CCM.CLOCK_ROOT25.DIV.scale" value="22" locked="false"/>
                  <setting id="CCM.CLOCK_ROOT25.MUX.sel" value="ANADIG_PLL.SYS_PLL2_CLK" locked="false"/>
                  <setting id="CCM.CLOCK_ROOT26.DIV.scale" value="22" locked="false"/>
                  <setting id="CCM.CLOCK_ROOT26.MUX.sel" value="ANADIG_PLL.SYS_PLL2_CLK" locked="false"/>
                  <setting id="CCM.CLOCK_ROOT3.DIV.scale" value="3" locked="false"/>
                  <setting id="CCM.CLOCK_ROOT3.MUX.sel" value="ANADIG_PLL.SYS_PLL3_CLK" locked="false"/>
                  <setting id="CCM.CLOCK_ROOT4.DIV.scale" value="3" locked="false"/>
                  <setting id="CCM.CLOCK_ROOT4.MUX.sel" value="ANADIG_PLL.SYS_PLL2_PFD1_CLK" locked="false"/>
                  <setting id="CCM.CLOCK_ROOT6.DIV.scale" value="4" locked="false"/>
                  <setting id="CCM.CLOCK_ROOT6.MUX.sel" value="ANADIG_PLL.SYS_PLL2_CLK" locked="false"/>
                  <setting id="CCM.CLOCK_ROOT68.DIV.scale" value="2" locked="false"/>
                  <setting id="CCM.CLOCK_ROOT68.MUX.sel" value="ANADIG_PLL.PLL_VIDEO_CLK" locked="false"/>
                  <setting id="CCM.CLOCK_ROOT8.DIV.scale" value="240" locked="false"/>
               </clock_settings>
               <called_from_default_init>true</called_from_default_init>
            </clock_configuration>
         </clock_configurations>
      </clocks>
      <dcdx name="DCDx" version="3.0" enabled="false" update_project_code="true">
         <generated_project_files/>
         <dcdx_profile>
            <processor_version>13.0.2</processor_version>
            <output_format>c_array</output_format>
         </dcdx_profile>
         <dcdx_configurations>
            <dcdx_configuration name="Device_configuration">
               <description></description>
               <options/>
               <command_groups>
                  <command_group name="Imported Commands" enabled="true">
                     <commands>
                        <command type="write_value" address="CCM_CLOCK_ROOT4_CONTROL" value="0x703" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B1_00" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B1_01" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B1_02" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B1_03" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B1_04" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B1_05" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B1_06" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B1_07" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B1_08" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B1_09" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B1_10" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B1_11" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B1_12" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B1_13" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B1_14" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B1_15" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B1_16" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B1_17" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B1_18" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B1_19" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B1_20" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B1_21" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B1_22" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B1_23" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B1_24" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B1_25" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B1_26" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B1_27" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B1_28" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B1_29" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B1_30" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B1_31" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B1_32" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B1_33" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B1_34" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B1_35" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B1_36" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B1_37" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B1_38" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B1_39" value="0x10" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B2_00" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B2_01" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B2_02" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B2_03" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B2_04" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B2_05" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B2_06" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B2_07" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B2_08" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B2_09" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B2_10" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B2_11" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B2_12" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B2_13" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B2_14" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B2_15" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B2_16" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_MUX_CTL_PAD_GPIO_EMC_B2_17" value="0x00" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B1_00" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B1_01" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B1_02" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B1_03" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B1_04" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B1_05" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B1_06" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B1_07" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B1_08" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B1_09" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B1_10" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B1_11" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B1_12" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B1_13" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B1_14" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B1_15" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B1_16" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B1_17" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B1_18" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B1_19" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B1_20" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B1_21" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B1_22" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B1_23" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B1_24" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B1_25" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B1_26" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B1_27" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B1_28" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B1_29" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B1_30" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B1_31" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B1_32" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B1_33" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B1_34" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B1_35" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B1_36" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B1_37" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B1_38" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B1_39" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B2_00" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B2_01" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B2_02" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B2_03" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B2_04" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B2_05" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B2_06" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B2_07" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B2_08" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B2_09" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B2_10" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B2_11" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B2_12" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B2_13" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B2_14" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B2_15" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B2_16" value="0x08" value_width="4"/>
                        <command type="write_value" address="IOMUXC_SW_PAD_CTL_PAD_GPIO_EMC_B2_17" value="0x08" value_width="4"/>
                        <command type="write_value" address="SEMC_MCR" value="0x10000004" value_width="4"/>
                        <command type="write_value" address="SEMC_BMCR0" value="0x81" value_width="4"/>
                        <command type="write_value" address="SEMC_BMCR1" value="0x81" value_width="4"/>
                        <command type="write_value" address="SEMC_BR0" value="0x8000001D" value_width="4"/>
                        <command type="write_value" address="SEMC_SDRAMCR0" value="0xF32" value_width="4"/>
                        <command type="write_value" address="SEMC_SDRAMCR1" value="0x772A22" value_width="4"/>
                        <command type="write_value" address="SEMC_SDRAMCR2" value="0x10A0D" value_width="4"/>
                        <command type="write_value" address="SEMC_SDRAMCR3" value="0x21210408" value_width="4"/>
                        <command type="write_value" address="SEMC_IPCR0" value="0x80000000" value_width="4"/>
                        <command type="write_value" address="SEMC_IPCR1" value="0x02" value_width="4"/>
                        <command type="write_value" address="SEMC_IPCR2" value="0x00" value_width="4"/>
                        <command type="write_value" address="SEMC_IPCMD" value="0xA55A000F" value_width="4"/>
                        <command type="nop"/>
                        <command type="nop"/>
                        <command type="nop"/>
                        <command type="nop"/>
                        <command type="nop"/>
                        <command type="write_value" address="SEMC_INTR" value="0x03" value_width="4"/>
                        <command type="write_value" address="SEMC_IPCMD" value="0xA55A000C" value_width="4"/>
                        <command type="nop"/>
                        <command type="nop"/>
                        <command type="nop"/>
                        <command type="nop"/>
                        <command type="nop"/>
                        <command type="write_value" address="SEMC_INTR" value="0x03" value_width="4"/>
                        <command type="write_value" address="SEMC_IPCMD" value="0xA55A000C" value_width="4"/>
                        <command type="nop"/>
                        <command type="nop"/>
                        <command type="nop"/>
                        <command type="nop"/>
                        <command type="nop"/>
                        <command type="write_value" address="SEMC_INTR" value="0x03" value_width="4"/>
                        <command type="write_value" address="SEMC_IPTXDAT" value="0x33" value_width="4"/>
                        <command type="write_value" address="SEMC_IPCMD" value="0xA55A000A" value_width="4"/>
                        <command type="nop"/>
                        <command type="nop"/>
                        <command type="nop"/>
                        <command type="nop"/>
                        <command type="nop"/>
                        <command type="write_value" address="SEMC_INTR" value="0x03" value_width="4"/>
                        <command type="write_value" address="SEMC_SDRAMCR3" value="0x21210409" value_width="4"/>
                     </commands>
                  </command_group>
               </command_groups>
            </dcdx_configuration>
         </dcdx_configurations>
      </dcdx>
      <periphs name="Peripherals" version="12.0" enabled="false" update_project_code="true">
         <dependencies>
            <dependency resourceType="SWComponent" resourceId="platform.drivers.lpuart" description="LPUART Driver not found in the toolchain/IDE project. Project will not compile!" problem_level="2" source="Peripherals">
               <feature name="enabled" evaluation="equal">
                  <data type="Boolean">true</data>
               </feature>
            </dependency>
            <dependency resourceType="SWComponent" resourceId="platform.drivers.lpuart" description="Unsupported version of the LPUART Driver in the toolchain/IDE project. Required: ${required_value}, actual: ${actual_value}. Project might not compile correctly." problem_level="1" source="Peripherals">
               <feature name="version" evaluation="equivalent">
                  <data type="Version">2.5.1</data>
               </feature>
            </dependency>
         </dependencies>
         <generated_project_files/>
         <peripherals_profile>
            <processor_version>13.0.2</processor_version>
         </peripherals_profile>
         <functional_groups>
            <functional_group name="BOARD_InitPeripherals" uuid="5580249f-8696-4d01-87fa-efd84baaea95" called_from_default_init="true" id_prefix="" core="cm7">
               <description></description>
               <options/>
               <dependencies>
                  <dependency resourceType="ClockOutput" resourceId="LPUART1_CLK_ROOT" description="LPUART1 clock root is inactive." problem_level="2" source="Peripherals:BOARD_InitPeripherals">
                     <feature name="frequency" evaluation="greaterThan">
                        <data type="Frequency" unit="Hz">0</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PeripheralUnifiedSignal" resourceId="LPUART1.uart_tx" description="Signal TX is not routed." problem_level="1" source="Peripherals:BOARD_InitPeripherals">
                     <feature name="routed" evaluation="equal">
                        <data type="Boolean">true</data>
                     </feature>
                  </dependency>
                  <dependency resourceType="PeripheralUnifiedSignal" resourceId="LPUART1.uart_rx" description="Signal RX is not routed." problem_level="1" source="Peripherals:BOARD_InitPeripherals">
                     <feature name="routed" evaluation="equal">
                        <data type="Boolean">true</data>
                     </feature>
                  </dependency>
               </dependencies>
               <instances>
                  <instance name="NVIC" uuid="27e59fb2-3864-4b83-bf0e-a683a8582c73" type="nvic" type_id="nvic_57b5eef3774cc60acaede6f5b8bddc67" mode="general" peripheral="NVIC" enabled="true" comment="" custom_name_enabled="false" editing_lock="false">
                     <config_set name="nvic">
                        <array name="interrupt_table"/>
                        <array name="interrupts"/>
                     </config_set>
                  </instance>
                  <instance name="LPUART1" uuid="78f9b1b2-5105-4480-a25a-29d8172b6270" type="lpuart" type_id="lpuart_bf01db7d964092f3cf860852cba17f7e" mode="polling" peripheral="LPUART1" enabled="true" comment="" custom_name_enabled="false" editing_lock="false">
                     <config_set name="lpuartConfig_t" quick_selection="QuickSelection1">
                        <struct name="lpuartConfig">
                           <setting name="clockSource" value="LpuartClock"/>
                           <setting name="lpuartSrcClkFreq" value="ClocksTool_DefaultInit"/>
                           <setting name="baudRate_Bps" value="115200"/>
                           <setting name="parityMode" value="kLPUART_ParityDisabled"/>
                           <setting name="dataBitsCount" value="kLPUART_EightDataBits"/>
                           <setting name="isMsb" value="false"/>
                           <setting name="stopBitCount" value="kLPUART_OneStopBit"/>
                           <setting name="enableMatchAddress1" value="false"/>
                           <setting name="matchAddress1" value="0"/>
                           <setting name="enableMatchAddress2" value="false"/>
                           <setting name="matchAddress2" value="0"/>
                           <setting name="txFifoWatermark" value="0"/>
                           <setting name="rxFifoWatermark" value="1"/>
                           <setting name="enableRxRTS" value="false"/>
                           <setting name="enableTxCTS" value="false"/>
                           <setting name="txCtsSource" value="kLPUART_CtsSourcePin"/>
                           <setting name="txCtsConfig" value="kLPUART_CtsSampleAtStart"/>
                           <setting name="rxIdleType" value="kLPUART_IdleTypeStartBit"/>
                           <setting name="rxIdleConfig" value="kLPUART_IdleCharacter1"/>
                           <setting name="enableTx" value="true"/>
                           <setting name="enableRx" value="true"/>
                        </struct>
                     </config_set>
                  </instance>
               </instances>
            </functional_group>
         </functional_groups>
         <components>
            <component name="system" uuid="cd2726b0-9595-440c-9375-bb6a010a1d55" type_id="system_54b53072540eeeb8f8e9343e71f28176">
               <config_set_global name="global_system_definitions">
                  <setting name="user_definitions" value=""/>
                  <setting name="user_includes" value=""/>
               </config_set_global>
            </component>
            <component name="msg" uuid="2491c39d-c21a-45f3-a984-57be0f6a77b5" type_id="msg_6e2baaf3b97dbeef01c0043275f9a0e7">
               <config_set_global name="global_messages"/>
            </component>
            <component name="gpio_adapter_common" uuid="fefc514e-ed7f-48ad-a874-de332dd5eb13" type_id="gpio_adapter_common_57579b9ac814fe26bf95df0a384c36b6">
               <config_set_global name="global_gpio_adapter_common" quick_selection="default"/>
            </component>
            <component name="generic_uart" uuid="1dc54607-ada6-4731-ad75-479a19616c00" type_id="generic_uart_8cae00565451cf2346eb1b8c624e73a6">
               <config_set_global name="global_uart"/>
            </component>
            <component name="generic_can" uuid="88660053-1bc1-49b8-884c-a12532e98a7a" type_id="generic_can_1bfdd78b1af214566c1f23cf6a582d80">
               <config_set_global name="global_can"/>
            </component>
            <component name="uart_cmsis_common" uuid="9d37100d-c1fb-4f7e-b235-a952c5b03275" type_id="uart_cmsis_common_9cb8e302497aa696fdbb5a4fd622c2a8">
               <config_set_global name="global_USART_CMSIS_common" quick_selection="default"/>
            </component>
            <component name="generic_enet" uuid="ad9ccf5d-6535-4f75-bb23-abb7e6fcc950" type_id="generic_enet_74db5c914f0ddbe47d86af40cb77a619">
               <config_set_global name="global_enet"/>
            </component>
         </components>
      </periphs>
      <tee name="TEE" version="4.0" enabled="false" update_project_code="true">
         <generated_project_files/>
         <tee_profile>
            <processor_version>N/A</processor_version>
         </tee_profile>
      </tee>
   </tools>
</configuration>
