# config/binary - options for live-build(7), binary stage

# Set image type
LB_IMAGE_TYPE="iso-hybrid"

# Set image filesystem
LB_BINARY_FILESYSTEM="fat32"

# Set apt/aptitude generic indices
LB_APT_INDICES="false"

# Set boot parameters
LB_BOOTAPPEND_LIVE="boot=live components console=tty0 console=ttyS0,115200n8 loglevel=4"

# Set boot parameters
LB_BOOTAPPEND_INSTALL=""

# Set boot parameters
LB_BOOTAPPEND_LIVE_FAILSAFE="boot=live components memtest noapic noapm nodma nomce nosmp nosplash vga=788"

# Set BIOS bootloader
LB_BOOTLOADER_BIOS="syslinux"

# Set EFI bootloader
LB_BOOTLOADER_EFI="grub-efi"

# Set bootloaders
LB_BOOTLOADERS=""

# Set checksums
LB_CHECKSUMS="sha256"

# Set compression
LB_COMPRESSION="none"

# Support dm-verity on rootfs
LB_DM_VERITY=""

# Support FEC on dm-verity rootfs
LB_DM_VERITY_FEC_ROOTS=""

# Set sign script for roothash for dm-verity rootfs
LB_DM_VERITY_SIGN=""

# Set zsync
LB_ZSYNC="false"

# Control if we build binary images chrooted
# NEVER, *EVER*, *E*V*E*R* SET THIS OPTION to false.
LB_BUILD_WITH_CHROOT="true"

# Set debian-installer
LB_DEBIAN_INSTALLER="none"

# Set debian-installer suite
LB_DEBIAN_INSTALLER_DISTRIBUTION="stable"

# Set debian-installer preseed filename/url
LB_DEBIAN_INSTALLER_PRESEEDFILE=""

# Toggle use of GUI debian-installer
LB_DEBIAN_INSTALLER_GUI="true"

# Set hdd label
LB_HDD_LABEL="DEBIAN_LIVE"

# Set hdd filesystem size
LB_HDD_SIZE="auto"

# Set start of partition for the hdd target for BIOSes that expect a specific boot partition start (e.g. "63s"). If empty, use optimal layout.
LB_HDD_PARTITION_START=""

# Set iso author
LB_ISO_APPLICATION="n-OS-tr"

# Set iso preparer
LB_ISO_PREPARER="live-build @LB_VERSION@; https://salsa.debian.org/live-team/live-build"

# Set iso publisher
LB_ISO_PUBLISHER="n-OS-tr project"

# Set iso volume (max 32 chars)
LB_ISO_VOLUME="n-OS-tr"

# Set jffs2 eraseblock size
LB_JFFS2_ERASEBLOCK=""

# Set memtest
LB_MEMTEST="none"

# Set loadlin
LB_LOADLIN="false"

# Set win32-loader
LB_WIN32_LOADER="false"

# Set net tarball
LB_NET_TARBALL="true"

# Set onie
LB_ONIE="false"

# Set onie additional kernel cmdline options
LB_ONIE_KERNEL_CMDLINE=""

# Set inclusion of firmware packages in debian-installer
LB_FIRMWARE_BINARY="true"

# Set inclusion of firmware packages in the live image
LB_FIRMWARE_CHROOT="true"

# Set swap file path
LB_SWAP_FILE_PATH=""

# Set swap file size
LB_SWAP_FILE_SIZE="512"

# Enable/disable UEFI secure boot support
LB_UEFI_SECURE_BOOT="auto"
